|  |  |
| --- | --- |
| Metro Welding Supply Corp. logo | Safety Data Sheet1-Pentene |
|  |

# Section 1: Product and Company Identification

**Metro Welding Supply Corp.**

12620 Southfield Road

Detroit, MI 48223

(313) 834-1660 [phone]

(313) 835-3562 [fax]

http://www.metrowelding.com/

Product Code: 1-Pentene

# Section 2: Hazards Identification



**Danger**

## Hazard Classification:

Aspiration Hazard (Category 1)

Flammable (Category 1)

Gases Under Pressure

## Hazard Statements:

Contains gas under pressure; may explode if heated

Extremely flammable gas

May be fatal if swallowed and enters airways

## Precautionary Statements

**Prevention:**

Keep away from heat/sparks/open flames/hot surfaces. - No smoking.

**Response:**

Do NOT induce vomiting.

Eliminate all ignition sources if safe to do so.

If swallowed: Rinse mouth. Do NOT induce vomiting.

Immediately call a poison center or doctor.

Leaking gas fire: Do not extinguish, unless leak can be stopped safely.

**Storage:**

Protect from sunlight.

Store in well-ventilated place.

Store locked up.

**Disposal:**

Dispose of contents and/or container in accordance with applicable regulations.

# Section 3: Composition/Information on Ingredients

| CAS # |
| --- |
| 109-67-1 |

| Chemical Substance | Chemical Family | Trade Names |
| --- | --- | --- |
| 1-PENTENE | hydrocarbons, aliphatic | ALPHA-N-AMYLENE; PROPYLETHYLENE; PENTENE; AMYLENE; UN 1108; C5H10 |

# Section 4: First Aid Measures

| Skin Contact | Eye Contact | Ingestion | Inhalation | Note to Physicians |
| --- | --- | --- | --- | --- |
| Wash skin with soap and water for at least 15 minutes while removing contaminated clothing and shoes. Get medical attention, if needed. Thoroughly clean and dry contaminated clothing and shoes before reuse. | Flush eyes with plenty of water for at least 15 minutes. Then get immediate medical attention. | Get medical attention immediately. | If adverse effects occur, remove to uncontaminated area. Give artificial respiration if not breathing. If breathing is difficult, oxygen should be administered by qualified personnel. Get immediate medical attention. | For inhalation, consider oxygen. For ingestion, consider gastric lavage. |

# Section 5: Fire Fighting Measures

| Suitable Extinguishing Media | Products of Combustion | Protection of Firefighters |
| --- | --- | --- |
| Alcohol resistant foam, carbon dioxide, regular dry chemical, water Large fires: Use alcohol-resistant foam or flood with fine water spray. | Carbon monoxide, carbon dioxide | * Any self-contained breathing apparatus that has a full facepiece and is operated in a pressure-demand or other positive-pressure mode.
* Any supplied-air respirator with full facepiece and operated in a pressure-demand or other positive-pressure mode in combination with a separate escape supply.
 |

# Section 6: Accidental Release Measures

| Personal Precautions | Environmental Precautions | Methods for Containment |
| --- | --- | --- |
| Keep unnecessary people away, isolate hazard area and deny entry. Stay upwind and keep out of low areas. | Avoid heat, flames, sparks and other sources of ignition. | Stop leak if possible without personal risk. Reduce vapors with water spray. Remove sources of ignition. |

| Methods for Cleanup | Other Information |
| --- | --- |
| Small spills: Absorb with sand or other non-combustible material. Collect spilled material in appropriate container for disposal. Large spills: Dike for later disposal. | None |

# Section 7: Handling and Storage

| Handling | Storage |
| --- | --- |
| Grounding and bonding required. Keep separated from incompatible substances. | Store and handle in accordance with all current regulations and standards. Subject to storage regulations: U.S. OSHA 29 CFR 1910.106. |

# Section 8: Exposure Controls/Personal Protection

| Exposure Guidelines |
| --- |
| 1-PENTENE: No occupational exposure limits established. |

## Engineering Controls

Handle only in fully enclosed systems.

| Eye Protection | Skin Protection | Respiratory Protection |
| --- | --- | --- |
| Wear splash resistant safety goggles. Provide an emergency eye wash fountain and quick drench shower in the immediate work area. | Wear appropriate chemical resistant clothing. |  Any self-contained breathing apparatus that has a full facepiece and is operated in a pressure-demand or other positive-pressure mode. |

## General Hygiene considerations

* Avoid breathing vapor or mist
* Avoid contact with eyes and skin
* Wash thoroughly after handling and before eating or drinking

# Section 9: Physical and Chemical Properties

| Physical State | Appearance | Color | Change in Appearance | Physical Form | Odor | Taste |
| --- | --- | --- | --- | --- | --- | --- |
| Liquid | Colorless | Colorless | N/A | Liquid | Unpleasant odor | N/A |

| Flash Point | Flammability | Partition Coefficient | Autoignition Temperature | Upper Explosive Limits | Lower Explosive Limits |
| --- | --- | --- | --- | --- | --- |
| -18 F (-28 C) (CC) | IA |  | 527 F (275 C) | 0.087 | 0.015 |

| Boiling Point | Freezing Point | Vapor Pressure | Vapor Density | Specific Gravity | Water Solubility | pH | Odor Threshold | Evaporation Rate | Viscosity |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 86 F (30 C) | -265 F (-165 C) | 495 mmHg @ 18 C | 2.4 (Air=1) | 0.6405 | Insoluble | Not available | 0.19 ppm | Not available | Not available |

| Molecular Weight | Molecular Formula | Density | Weight per Gallon | Volatility by Volume | Volatility | Solvent Solubility |
| --- | --- | --- | --- | --- | --- | --- |
| 70.13 | C-H3-(C-H2)2-C-H-C-H2 | Not available | Not available | Not available | Not available | Soluble: Alcohol, ether, benzene |

# Section 10: Stability and Reactivity

| Stability | Conditions to Avoid | Incompatible Materials |
| --- | --- | --- |
| Stable at normal temperatures and pressure. May form explosive peroxides. Avoid contact with air, light or storage and use above room temperature. | Stable at normal temperatures and pressure. May form explosive peroxides. Avoid contact with air, light or storage and use above room temperature. | Oxidizing materials, halogens, acids |

| Hazardous Decomposition Products | Possibility of Hazardous Reactions |
| --- | --- |
| Oxides of carbon. May form explosive, shock- and heat-sensitive organic peroxides when exposed to air.  | Will not polymerize. |

# Section 11: Toxicology Information

## Acute Effects

| Oral LD50 | Dermal LD50 | Inhalation |
| --- | --- | --- |
| Inhalation LC50 Rat 175000 mg/m3 4 h | Not established | Irritation, nausea, vomiting, symptoms of drunkenness, suffocation, convulsions, coma |

| Eye Irritation | Skin Irritation | Sensitization |
| --- | --- | --- |
| Irritation | Irritation | Respiratory tract irritation, skin irritation, eye irritation, central nervous system depression, difficulty breathing |

## Chronic Effects

| Carcinogenicity | Mutagenicity | Reproductive Effects | Developmental Effects |
| --- | --- | --- | --- |
| Not listed. | Not established | Not established | No data |

# Section 12: Ecological Information

## Fate and Transport

|  |  |  |  |
| --- | --- | --- | --- |
| Eco toxicity | Persistence / Degradability | Bioaccumulation / Accumulation | Mobility in Environment |
| Fish toxicity: Not availableInvertibrate toxicity: Not availableAlgal toxicity: Not availablePhyto toxicity: Not availableOther toxicity: Not available | Not available | Not available | Not available |

# Section 13: Disposal Considerations

|  |
| --- |
| Subject to disposal regulations: U.S. EPA 40 CFR 262. Hazardous Waste Number(s): D001. Dispose in accordance with all applicable regulations. |

# Section 14: Transportation Information

## U.S. DOT 49 CFR 172.101

| Proper Shipping Name | ID Number | Hazard Class or Division | Packing Group | Labeling Requirements | Passenger Aircraft or Railcar Quantity Limitations | Cargo Aircraft Only Quantity Limitations | Additional Shipping Description |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1-Pentene | UN1108 | 3 | I | 3 | 1 kg or L | 30 L | N/A |

## Canadian Transportation of Dangerous Goods

|  |  |  |  |
| --- | --- | --- | --- |
| Shipping Name | UN Number | Class | Packing Group / Risk Group |
| 1-PENTENE (n-amylene) | UN1108 | 3 | I |

# Section 15: Regulatory Information

## U.S. Regulations

|  |  |  |
| --- | --- | --- |
| CERCLA Sections | SARA 355.30 | SARA 355.40 |
| Not regulated. | Not regulated. | Not regulated. |

## SARA 370.21

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Acute | Chronic | Fire | Reactive | Sudden Release |
| Yes | No | Yes | No | No |

## SARA 372.65

|  |
| --- |
| Not regulated. |

## OSHA Process Safety

|  |
| --- |
| Not regulated. |

## State Regulations

|  |
| --- |
| CA Proposition 65 |
| Not regulated. |

## Canadian Regulations

|  |
| --- |
| WHMIS Classification |
| B |

## National Inventory Status

|  |  |  |
| --- | --- | --- |
| US Inventory (TSCA) | TSCA 12b Export Notification | Canada Inventory (DSL/NDSL) |
| Listed on inventory. | Not listed. | Not determined. |

# Section 16: Other Information

|  |
| --- |
| NFPA Rating |
| HEALTH=2 FIRE=4 REACTIVITY=0 |

0 = minimal hazard, 1 = slight hazard, 2 = moderate hazard, 3 = severe hazard, 4 = extreme hazard