|  |  |
| --- | --- |
| Metro Welding Supply Corp. logo | Safety Data SheetAcetylene |
|  |

# Section 1: Product and Company Identification

**Metro Welding Supply Corp.**

12620 Southfield Road

Detroit, MI 48223

(313) 834-1660 [phone]

(313) 835-3562 [fax]

http://www.metrowelding.com/

Product Code: Acetylene

# Section 2: Hazards Identification



**Danger**

## Hazard Classification:

Flammable (Category 1)

Gases Under Pressure

## Hazard Statements:

Contains gas under pressure; may explode if heated

Extremely flammable gas

## Precautionary Statements

**Prevention:**

Keep away from heat/sparks/open flames/hot surfaces. - No smoking.

**Response:**

Eliminate all ignition sources if safe to do so.

Leaking gas fire: Do not extinguish, unless leak can be stopped safely.

**Storage:**

Protect from sunlight.

Store in well-ventilated place.

# Section 3: Composition/Information on Ingredients

| CAS # |
| --- |
| 74-86-2 |

| Chemical Substance | Chemical Family | Trade Names |
| --- | --- | --- |
| ACETYLENE, DISSOLVED | hydrocarbons, aliphatic | ACETYLENE; ETHYNE; WELDING GAS; ACETYLEN; ETHINE; NARCYLEN; VINYLENE; UN 1001; C2H2 |

# Section 4: First Aid Measures

| Skin Contact | Eye Contact | Ingestion | Inhalation | Note to Physicians |
| --- | --- | --- | --- | --- |
| Gas: Not applicable. Liquid: Wash exposed skin with soap and water. | Gas: Not applicable. Liquid: Flush eyes with plenty of water. | Not applicable. | If adverse effects occur, remove to uncontaminated area. Give artificial respiration if not breathing. If breathing is difficult, oxygen should be administered by qualified personnel. Get immediate medical attention. | For inhalation, consider oxygen. |

# Section 5: Fire Fighting Measures

| Suitable Extinguishing Media | Products of Combustion | Protection of Firefighters |
| --- | --- | --- |
| Carbon dioxide, regular dry chemical Large fires: Use regular foam or flood with fine water spray. | Oxides of carbon | * Respiratory protection may be needed for frequent or heavy exposure.
* Any self-contained breathing apparatus with a full facepiece.
 |

# Section 6: Accidental Release Measures

| Personal Precautions | Environmental Precautions | Methods for Containment |
| --- | --- | --- |
| Keep unnecessary people away, isolate hazard area and deny entry. Ventilate closed spaces before entering. | Avoid heat, flames, sparks and other sources of ignition. | Stop leak if possible without personal risk. Reduce vapors with water spray. Remove sources of ignition. |

| Methods for Cleanup | Other Information |
| --- | --- |
| Evacuate, stop leak if possible. Remove sources of ignition.  | None |

# Section 7: Handling and Storage

| Handling | Storage |
| --- | --- |
| Avoid heat, flames, sparks and other sources of ignition. Grounding and bonding required. Secure to prevent tipping. Subject to storage regulations: U.S. OSHA 29 CFR 1910.101. Keep separated from incompatible substances. | Store and handle in accordance with all current regulations and standards. Protect from physical damage. Store outside or in a detached building. Keep separated from incompatible substances. Store in a cool, dry place. Store in a well-ventilated area.  |

# Section 8: Exposure Controls/Personal Protection

| Exposure Guidelines |
| --- |
| ACETYLENE, DISSOVED: ACETYLENE: ACGIH (simple asphyxiant) 2500 ppm (2662 mg/m3) NIOSH recommended ceiling |

## Engineering Controls

Handle only in fully enclosed systems.

| Eye Protection | Skin Protection | Respiratory Protection |
| --- | --- | --- |
| Eye protection not required, but recommended. | Protective clothing is not required. | Respiratory protection may be needed for frequent or heavy exposure. |

## General Hygiene considerations

* Avoid breathing vapor or mist
* Avoid contact with eyes and skin
* Wash thoroughly after handling and before eating or drinking

# Section 9: Physical and Chemical Properties

| Physical State | Appearance | Color | Change in Appearance | Physical Form | Odor | Taste |
| --- | --- | --- | --- | --- | --- | --- |
| Gas | Colorless | Colorless | N/A | Liquefied gas | Sweet odor | N/A |

| Flash Point | Flammability | Partition Coefficient | Autoignition Temperature | Upper Explosive Limits | Lower Explosive Limits |
| --- | --- | --- | --- | --- | --- |
| Flammable gas. Can be ignited at all normal temperatures. A flash point of 0 F (-18 C) (CC) has been reported. |  | 2691.53 (log = 3.44) (estimated from water solubility) | 581 F (305 C) | 81%; 100% if there is a substantial energy ignition source, and under certain conditions of pressure, container size and shape.‘ | 0.025 |

| Boiling Point | Freezing Point | Vapor Pressure | Vapor Density | Specific Gravity | Water Solubility | pH | Odor Threshold | Evaporation Rate | Viscosity |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| -103 F (-75 C) @ 170 kPa abs (24.7 psi abs) or 69 kPa gage (10 psi gage) | Not available | 760 mmHg @ -84 C | 0.9 (Air=1) | Not applicable | 0.94% @ 25 C | Not applicable | 240 mg/m3 (226 ppm) (detection) (4); 657 mg/m3 (620 ppm) (not specified) (8) 1300-2750 mg/m3 (1222-2585 ppm) (not specified) | Not applicable | 0.010 cP @ 20 C |

| Molecular Weight | Molecular Formula | Density | Weight per Gallon | Volatility by Volume | Volatility | Solvent Solubility |
| --- | --- | --- | --- | --- | --- | --- |
| 26.04 | H-C-C-H | 1.1747 g/L @ 0 C | Not available | Not available | Not applicable | Soluble: Acetone, benzene, chloroform, ether |

# Section 10: Stability and Reactivity

| Stability | Conditions to Avoid | Incompatible Materials |
| --- | --- | --- |
| May decompose violently on heating. May explode when heated. | May decompose violently on heating. May explode when heated. | Metals, halogens, oxidizing materials, metal carbide, reducing agents, halo carbons
BRASS. CALCIUM HYPOCHLORITE, COPPER, MERCURY AND SILVER SALTS, HALOGENS, HEAVY METALS, HYDRIDES, LIQUID NITROGEN, NITRIC ACID , OXYGEN, OZONE, PERCHLORIC ACID, POTASSIUM  |

| Hazardous Decomposition Products | Possibility of Hazardous Reactions |
| --- | --- |
| Hydrogen | Polymerizes with evolution of heat. Avoid contact with curing agents, accelerators, and/or initiators. |

# Section 11: Toxicology Information

## Acute Effects

| Oral LD50 | Dermal LD50 | Inhalation |
| --- | --- | --- |
| Not established | Not established | Nausea, vomiting, chest pain, wheezing, headache, drowsiness, dizziness, loss of coordination, bluish skin color, suffocation, lung congestion, coma |

| Eye Irritation | Skin Irritation | Sensitization |
| --- | --- | --- |
| No information on significant adverse effects | Rash | Central nervous system depression, difficulty breathing, asphyxiant |

## Chronic Effects

| Carcinogenicity | Mutagenicity | Reproductive Effects | Developmental Effects |
| --- | --- | --- | --- |
| Not established | Not established | Not established | No data |

# Section 12: Ecological Information

## Fate and Transport

|  |  |  |  |
| --- | --- | --- | --- |
| Eco toxicity | Persistence / Degradability | Bioaccumulation / Accumulation | Mobility in Environment |
| Fish toxicity: Not availableInvertibrate toxicity: Not availableAlgal toxicity: Not availablePhyto toxicity: Not availableOther toxicity: Not available | Relatively non-persistent in the environment. Highly volatile from water. | Accumulates very little in the bodies of living organisms. | Not expected to leach through the soil or the sediment. |

# Section 13: Disposal Considerations

|  |
| --- |
| Dispose in accordance with all applicable regulations. Subject to disposal regulations: U.S. EPA 40 CFR 262. Hazardous Waste Number(s): D001. D003. |

# Section 14: Transportation Information

## U.S. DOT 49 CFR 172.101

| Proper Shipping Name | ID Number | Hazard Class or Division | Packing Group | Labeling Requirements | Passenger Aircraft or Railcar Quantity Limitations | Cargo Aircraft Only Quantity Limitations | Additional Shipping Description |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Acetylene, dissolved | UN1001 | 2.1 | Not applicable | 2.1 | Forbidden | 15 kg | N/A |

## Canadian Transportation of Dangerous Goods

|  |  |  |  |
| --- | --- | --- | --- |
| Shipping Name | UN Number | Class | Packing Group / Risk Group |
| Acetylene, dissolved | UN1001 | 2.1 | Not applicable |

# Section 15: Regulatory Information

## U.S. Regulations

|  |  |  |
| --- | --- | --- |
| CERCLA Sections | SARA 355.30 | SARA 355.40 |
| Not regulated. | Not regulated. | Not regulated. |

## SARA 370.21

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Acute | Chronic | Fire | Reactive | Sudden Release |
| Yes | No | Yes | Yes | Yes |

## SARA 372.65

|  |
| --- |
| Not regulated. |

## OSHA Process Safety

|  |
| --- |
| Not regulated. |

## State Regulations

|  |
| --- |
| CA Proposition 65 |
| Not regulated. |

## Canadian Regulations

|  |
| --- |
| WHMIS Classification |
| A, B1 |

## National Inventory Status

|  |  |  |
| --- | --- | --- |
| US Inventory (TSCA) | TSCA 12b Export Notification | Canada Inventory (DSL/NDSL) |
| Listed on inventory. | Not listed. | Not determined. |

# Section 16: Other Information

|  |
| --- |
| NFPA Rating |
| HEALTH=1 FIRE=4 REACTIVITY=3 |

0 = minimal hazard, 1 = slight hazard, 2 = moderate hazard, 3 = severe hazard, 4 = extreme hazard