|  |  |
| --- | --- |
| Metro Welding Supply Corp. logo | Safety Data SheetHeptane |
|  |

# Section 1: Product and Company Identification

**Metro Welding Supply Corp.**

12620 Southfield Road

Detroit, MI 48223

(313) 834-1660 [phone]

(313) 835-3562 [fax]

http://www.metrowelding.com/

Product Code: Heptane

# Section 2: Hazards Identification



**Danger**

## Hazard Classification:

Acute Gas Inhale Toxicity (Category 2)

Acute Oral Toxicity (Category 3)

Eye Effects (Category 2.B)

Flammable (Category 1)

Flammable Aerosol (Category 1)

Gases Under Pressure

## Hazard Statements:

Causes eye irritation

Contains gas under pressure; may explode if heated

Extremely flammable aerosol

Extremely flammable gas

Fatal if inhaled

Toxic if swallowed

## Precautionary Statements

**Prevention:**

Wash thoroughly after handling.

Do not eat, drink or smoke when using this product.

[In case of inadequate ventilation] wear respiratory protection.

Do not breathe dust/fume/gas/mist/ vapors/spray..

Use only outdoors or in a well-ventilated area.

Keep away from heat/sparks/open flames/hot surfaces. - No smoking.

Pressurized container: Do not pierce or burn, even after use.

Do not spray on an open flame or other ignition source.

**Response:**

Eliminate all ignition sources if safe to do so.

Immediately call a poison center or doctor.

Leaking gas fire: Do not extinguish, unless leak can be stopped safely.

Specific treatment is urgent.

If swallowed: Rinse mouth. Do NOT induce vomiting.

If in eyes: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing.

If inhaled: Remove person to fresh air and keep comfortable for breathing.

**Storage:**

Store in a well-ventilated place. Keep container tightly closed.

Protect from sunlight.

Store locked up.

Do not expose to temperatures exceeding 50C/122F.

**Disposal:**

Dispose of contents and/or container in accordance with applicable regulations.

# Section 3: Composition/Information on Ingredients

| CAS # |
| --- |
| 142-82-5 |

| Chemical Substance | Chemical Family | Trade Names |
| --- | --- | --- |
| n-HEPTANE | hydrocarbons, aliphatic | NORMAL HEPTANE; DIPROPYL METHANE; HEPTYL HYDRIDE; DIPROPYLMETHANE; N-HEPTANE; UN 1206; C7H16 |

# Section 4: First Aid Measures

| Skin Contact | Eye Contact | Ingestion | Inhalation | Note to Physicians |
| --- | --- | --- | --- | --- |
| Wash skin with soap and water for at least 15 minutes while removing contaminated clothing and shoes. Get medical attention, if needed. Thoroughly clean and dry contaminated clothing and shoes before reuse. | Immediately flush eyes with plenty of water for at least 15 minutes. Then get immediate medical attention. | Aspiration hazard. DO NOT induce vomiting. If vomiting occurs, keep head lower than hips to help prevent aspiration. Get immediate medical attention. Give artificial respiration if not breathing. | If adverse effects occur, remove to uncontaminated area. Give artificial respiration if not breathing. Get immediate medical attention. | Not Available |

# Section 5: Fire Fighting Measures

| Suitable Extinguishing Media | Products of Combustion | Protection of Firefighters |
| --- | --- | --- |
| Regular dry chemical, carbon dioxide, water, regular foam Large fires: Use regular foam or flood with fine water spray. | Irritating, toxic gases | * Any self-contained breathing apparatus that has a full facepiece and is operated in a pressure-demand or other positive-pressure mode.
* Any self-contained breathing apparatus that has a full facepiece and is operated in a pressure-demand or other positive-pressure mode.
 |

# Section 6: Accidental Release Measures

| Personal Precautions | Environmental Precautions | Methods for Containment |
| --- | --- | --- |
| Keep unnecessary people away, isolate hazard area and deny entry. | Avoid heat, flames, sparks and other sources of ignition. | Stop leak if possible without personal risk. Reduce vapors with water spray. Remove sources of ignition. |

| Methods for Cleanup | Other Information |
| --- | --- |
| Small spills: Absorb with sand or other non-combustible material. Collect spilled material in appropriate container for disposal. Large spills: Dike for later disposal. Remove | None |

# Section 7: Handling and Storage

| Handling | Storage |
| --- | --- |
| Store and handle in accordance with all current regulations and standards. Subject to storage regulations: U.S. OSHA 29 CFR 1910.106.  | Grounding and bonding required. Keep separated from incompatible substances. |

# Section 8: Exposure Controls/Personal Protection

| Exposure Guidelines |
| --- |
| HEPTANE: n-HEPTANE: 500 ppm (2000 mg/m3) OSHA TWA 400 ppm (1640 mg/m3) OSHA TWA (vacated by 58 FR 35338, June 30, 1993) 500 ppm (2050 mg/m3) OSHA STEL (vacated by 58 FR 35338, June 30, 1993) 85 ppm (350 mg/m3) NIOSH recommended TWA 10 hour(s) 440 ppm (1800 mg/m3) NIOSH recommended ceiling 15 minute(s) HEPTANE, ALL ISOMERS: 400 ppm ACGIH TWA 500 ppm ACGIH STEL |

## Engineering Controls

Handle only in fully enclosed systems.

| Eye Protection | Skin Protection | Respiratory Protection |
| --- | --- | --- |
| Wear splash resistant safety goggles. Provide an emergency eye wash fountain and quick drench shower in the immediate work area. | Wear appropriate chemical resistant clothing. | Any self-contained breathing apparatus that has a full facepiece and is operated in a pressure-demand or other positive-pressure mode.  |

## General Hygiene considerations

* Avoid breathing vapor or mist
* Avoid contact with eyes and skin
* Wash thoroughly after handling and before eating or drinking

# Section 9: Physical and Chemical Properties

| Physical State | Appearance | Color | Change in Appearance | Physical Form | Odor | Taste |
| --- | --- | --- | --- | --- | --- | --- |
| Liquid | Clear | Colorless | N/A | Volatile liquid | Faint odor, gasoline odor | N/A |

| Flash Point | Flammability | Partition Coefficient | Autoignition Temperature | Upper Explosive Limits | Lower Explosive Limits |
| --- | --- | --- | --- | --- | --- |
| 25 F (-4 C) (CC) | IB | Not available | 399 F (204 C) | 0.067 | 0.0105 |

| Boiling Point | Freezing Point | Vapor Pressure | Vapor Density | Specific Gravity | Water Solubility | pH | Odor Threshold | Evaporation Rate | Viscosity |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 208 F (98 C) | -132 F (-91 C) | 40 mmHg @ 20 C | 3.45 (Air=1) | 0.6837 | 0.005% | Not available | 220 ppm | 2.80 (butyl acetate=1) | Not available |

| Molecular Weight | Molecular Formula | Density | Weight per Gallon | Volatility by Volume | Volatility | Solvent Solubility |
| --- | --- | --- | --- | --- | --- | --- |
| 100.21 | C-H3-(C-H2)5-C-H3 | Not available | Not available | Not available | 1 | Soluble: Ethanol, ether, chloroform, acetone |

# Section 10: Stability and Reactivity

| Stability | Conditions to Avoid | Incompatible Materials |
| --- | --- | --- |
| Stable at normal temperatures and pressure. | Stable at normal temperatures and pressure. | Oxidizing materials, combustible materials |

| Hazardous Decomposition Products | Possibility of Hazardous Reactions |
| --- | --- |
| Oxides of carbon | Will not polymerize. |

# Section 11: Toxicology Information

## Acute Effects

| Oral LD50 | Dermal LD50 | Inhalation |
| --- | --- | --- |
| 103 gm/m3/4 hour(s) inhalation-rat LC50 | Not available | Irritation, loss of appetite, headache, drowsiness, dizziness, emotional disturbances, loss of coordination, suffocation, unconsciousness |

| Eye Irritation | Skin Irritation | Sensitization |
| --- | --- | --- |
| Irritation | Irritation | Respiratory tract irritation, skin irritation, eye irritation, aspiration hazard, central nervous system depression |

## Chronic Effects

| Carcinogenicity | Mutagenicity | Reproductive Effects | Developmental Effects |
| --- | --- | --- | --- |
| Not available | Not available | Not available | No data |

# Section 12: Ecological Information

## Fate and Transport

|  |  |  |  |
| --- | --- | --- | --- |
| Eco toxicity | Persistence / Degradability | Bioaccumulation / Accumulation | Mobility in Environment |
| Fish toxicity: Acute LC50 4924000 ug/L Fresh water Fish - Western mosquitofish - Gambusia affinis - Adult 96 hours; 375000 ug/L 96 hour(s) LC50 (Mortality) MozambiquInvertibrate toxicity: 2500000 ug/L 96 hour(s) LC50 (Mortality) Oligochaete (Branchiura sowerbyi)Algal toxicity: 1500 ug/L 8 year(s) EC50 (Photosynthesis) Algae,phytoplankton,algal mat (Algae)Phyto toxicity: Not availableOther toxicity: Not available | Harmful to aquatic life. | Not available | Not available |

# Section 13: Disposal Considerations

|  |
| --- |
| Subject to disposal regulations: U.S. EPA 40 CFR 262. Hazardous Waste Number(s): D001. Dispose in accordance with all applicable regulations. |

# Section 14: Transportation Information

## U.S. DOT 49 CFR 172.101

| Proper Shipping Name | ID Number | Hazard Class or Division | Packing Group | Labeling Requirements | Passenger Aircraft or Railcar Quantity Limitations | Cargo Aircraft Only Quantity Limitations | Additional Shipping Description |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Heptanes | UN1206 | 3 | II | 3 | N/A | N/A | N/A |

## Canadian Transportation of Dangerous Goods

|  |  |  |  |
| --- | --- | --- | --- |
| Shipping Name | UN Number | Class | Packing Group / Risk Group |
| Heptanes | UN1206 | 3 | II |

# Section 15: Regulatory Information

## U.S. Regulations

|  |  |  |
| --- | --- | --- |
| CERCLA Sections | SARA 355.30 | SARA 355.40 |
| Not regulated. | Not regulated. | Not regulated. |

## SARA 370.21

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Acute | Chronic | Fire | Reactive | Sudden Release |
| Yes | No | Yes | No | No |

## SARA 372.65

|  |
| --- |
| Not regulated. |

## OSHA Process Safety

|  |
| --- |
| Not regulated. |

## State Regulations

|  |
| --- |
| CA Proposition 65 |
| Not regulated. |

## Canadian Regulations

|  |
| --- |
| WHMIS Classification |
| B2 D2B |

## National Inventory Status

|  |  |  |
| --- | --- | --- |
| US Inventory (TSCA) | TSCA 12b Export Notification | Canada Inventory (DSL/NDSL) |
| Listed on inventory. | HEPTANE CAS NUMBER: 142-82-5 SECTION 4 | Not determined. |

# Section 16: Other Information

|  |
| --- |
| NFPA Rating |
| HEALTH=2 FIRE=3 REACTIVITY=0 |

0 = minimal hazard, 1 = slight hazard, 2 = moderate hazard, 3 = severe hazard, 4 = extreme hazard