|  |  |
| --- | --- |
| Metro Welding Supply Corp. logo | Safety Data SheetHexane |
|  |

# Section 1: Product and Company Identification

**Metro Welding Supply Corp.**

12620 Southfield Road

Detroit, MI 48223

(313) 834-1660 [phone]

(313) 835-3562 [fax]

http://www.metrowelding.com/

Product Code: Hexane

# Section 2: Hazards Identification



**Danger**

## Hazard Classification:

Acute Dermal Toxicity (Category 1)

Acute Oral Toxicity (Category 2)

Aspiration Hazard (Category 1)

Eye Effects (Category 2.B)

Flammable (Category 1)

Flammable Aerosol (Category 1)

Gases Under Pressure

## Hazard Statements:

Causes eye irritation

Contains gas under pressure; may explode if heated

Extremely flammable aerosol

Extremely flammable gas

Fatal if swallowed

Fatal in contact with skin

May be fatal if swallowed and enters airways

Toxic to aquatic life

## Precautionary Statements

**Prevention:**

Wash thoroughly after handling.

Do not eat, drink or smoke when using this product.

Do not get in eyes, on skin, or on clothing.

Wear protective gloves and protective clothing.

Keep away from heat/sparks/open flames/hot surfaces. - No smoking.

Pressurized container: Do not pierce or burn, even after use.

Do not spray on an open flame or other ignition source.

**Response:**

Eliminate all ignition sources if safe to do so.

Immediately call a poison center or doctor.

Leaking gas fire: Do not extinguish, unless leak can be stopped safely.

Do NOT induce vomiting.

Take off immediately all contaminated clothing and wash it before reuse.

If swallowed: Rinse mouth. Do NOT induce vomiting.

If in eyes: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing.

Wash with plenty of water

**Storage:**

Protect from sunlight.

Store in well-ventilated place.

Store locked up.

Do not expose to temperatures exceeding 50C/122F.

**Disposal:**

Dispose of contents and/or container in accordance with applicable regulations.

# Section 3: Composition/Information on Ingredients

| CAS # |
| --- |
| 110-54-3 |

| Chemical Substance | Chemical Family | Trade Names |
| --- | --- | --- |
| HEXANE | hydrocarbons, aliphatic | N-HEXANE; 1-HEXANE; HEXYL HYDRIDE; 1-HEXANE; NORMAL HEXANE; SKELLYSOLVE B; UN 1208; CAPROYL HYDRIDE; C6H14 |

# Section 4: First Aid Measures

| Skin Contact | Eye Contact | Ingestion | Inhalation | Note to Physicians |
| --- | --- | --- | --- | --- |
| Wash skin with soap and water for at least 15 minutes while removing contaminated clothing and shoes. Get medical attention, if needed. Thoroughly clean and dry contaminated clothing and shoes before reuse. | Flush eyes with plenty of water for at least 15 minutes. Then get immediate medical attention. | Aspiration hazard. DO NOT induce vomiting. If vomiting occurs, keep head lower than hips to help prevent aspiration. Get immediate medical attention. Give artificial respiration if not breathing. | If adverse effects occur, remove to uncontaminated area. Give artificial respiration if not breathing. If breathing is difficult, oxygen should be administered by qualified personnel. Get immediate medical attention. | There is no specific antidote. Treatment of overexposure should be directed at the control of symptoms and the clinical condition of the patient. Long-term exposure to n-hexane can cause damage to the peripheral nervous system. |

# Section 5: Fire Fighting Measures

| Suitable Extinguishing Media | Products of Combustion | Protection of Firefighters |
| --- | --- | --- |
| Regular dry chemical, carbon dioxide, water, regular foam Large fires: Use regular foam or flood with fine water spray. | Carbon monoxide, carbon dioxide and toxic and irritating fumes | * Any appropriate escape-type, self-contained breathing apparatus.
* Protective material types: rubber
 |

# Section 6: Accidental Release Measures

| Personal Precautions | Environmental Precautions | Methods for Containment |
| --- | --- | --- |
| Keep unnecessary people away, isolate hazard area and deny entry. | Avoid heat, flames, sparks and other sources of ignition. | Stop leak if possible without personal risk. Reduce vapors with water spray. |

| Methods for Cleanup | Other Information |
| --- | --- |
| Small spills: Absorb with sand or other non-combustible material. Collect spilled material in appropriate container for disposal. Large spills: Dike for later disposal. Remove sources of ignition. | Notify Local Emergency Planning Committee and State Emergency Response Commission for release greater than or equal to RQ (U.S. SARA Section 304). If release occurs in the U.S. and is reportable under CERCLA Section 103, notify the National Response Center at (800)424-8802 (USA) or (202)426-2675 (USA). |

# Section 7: Handling and Storage

| Handling | Storage |
| --- | --- |
| Store and handle in accordance with all current regulations and standards. Store in a tightly closed container. Store in a well-ventilated area. Store in a cool, dry place. Subject to storage regulations: U.S. OSHA 29 CFR 1910.106. |  Grounding and bonding required. Keep separated from incompatible substances. |

# Section 8: Exposure Controls/Personal Protection

| Exposure Guidelines |
| --- |
| N-HEXANE: 500 ppm (1800 mg/m3) OSHA TWA 50 ppm (180 mg/m3) OSHA TWA (vacated by 58 FR 35338, June 30, 1993) 50 ppm ACGIH TWA (skin) 50 ppm (180 mg/m3) NIOSH recommended TWA 10 hour(s) |

## Engineering Controls

Handle only in fully enclosed systems.

| Eye Protection | Skin Protection | Respiratory Protection |
| --- | --- | --- |
| Wear splash resistant safety goggles with a face shield. Provide an emergency eye wash fountain and quick drench shower in the immediate work area. | Wear appropriate chemical resistant clothing. |  Any appropriate escape-type, self-contained breathing apparatus. |

## General Hygiene considerations

* Avoid breathing vapor or mist
* Avoid contact with eyes and skin
* Wash thoroughly after handling and before eating or drinking

# Section 9: Physical and Chemical Properties

| Physical State | Appearance | Color | Change in Appearance | Physical Form | Odor | Taste |
| --- | --- | --- | --- | --- | --- | --- |
| Liquid | Clear | Colorless | N/A | Liquid | Faint odor, gasoline odor | N/A |

| Flash Point | Flammability | Partition Coefficient | Autoignition Temperature | Upper Explosive Limits | Lower Explosive Limits |
| --- | --- | --- | --- | --- | --- |
| -9.4 F (-23 C) (CC); -7 F (-21.7 C) (CC) | IB | 139315.68 (log = 5.148) (estimated from water solubility) | 437 F (225 C) | 0.075 | 0.011 |

| Boiling Point | Freezing Point | Vapor Pressure | Vapor Density | Specific Gravity | Water Solubility | pH | Odor Threshold | Evaporation Rate | Viscosity |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 156 F (69 C) | -139 F (-95 C) | 124 mmHg @ 20 C | 3 (Air=1) | 0.6603 | 0.014% @ 20 C | Neutral | 64-244 ppm | 8.9 (n-butyl acetate = 1) | 0.32 cP @ 25 C |

| Molecular Weight | Molecular Formula | Density | Weight per Gallon | Volatility by Volume | Volatility | Solvent Solubility |
| --- | --- | --- | --- | --- | --- | --- |
| 86.18 | C-H3-(C-H2)4-C-H3 | Not available | Not available | Not available | 675 g/l VOC (w/v) | Soluble: Alcohol, ether, chloroform, acetone, organic solvents |

# Section 10: Stability and Reactivity

| Stability | Conditions to Avoid | Incompatible Materials |
| --- | --- | --- |
| Stable at normal temperatures and pressure. | Stable at normal temperatures and pressure. | Oxidizing materials, halogens, combustible materials, chlorine dioxide, fluorine, nitrogen dioxide, potassium chlorate, chlorine, chlorosulfuric acid |

| Hazardous Decomposition Products | Possibility of Hazardous Reactions |
| --- | --- |
| Oxides of carbon | Will not polymerize. |

# Section 11: Toxicology Information

## Acute Effects

| Oral LD50 | Dermal LD50 | Inhalation |
| --- | --- | --- |
| >5 gm/kg oral-rat LD50 | >2 gm/kg skin-rabbit LD50 | Irritation, nausea, irregular heartbeat, headache, drowsiness, dizziness, mood swings, loss of coordination, lung congestion, nerve damage, brain damage, unconsciousness |

| Eye Irritation | Skin Irritation | Sensitization |
| --- | --- | --- |
| Mild irritation | Irritation | Respiratory tract irritation, skin irritation, eye irritation, aspiration hazard, central nervous system depression, nerve damage, asphyxiant |

## Chronic Effects

| Carcinogenicity | Mutagenicity | Reproductive Effects | Developmental Effects |
| --- | --- | --- | --- |
| Not listed. | Available. | Available. | No data |

# Section 12: Ecological Information

## Fate and Transport

|  |  |  |  |
| --- | --- | --- | --- |
| Eco toxicity | Persistence / Degradability | Bioaccumulation / Accumulation | Mobility in Environment |
| Fish toxicity: 2500 ug/L 96 hour(s) LC50 (Mortality) Fathead minnow (Pimephales promelas)Invertibrate toxicity: Not availableAlgal toxicity: 75 ug/L 28 hour(s) (Population Growth) Green algae (Chlamydomonas sp)Phyto toxicity: Not availableOther toxicity: Not available | Relatively non-persistent in the environment. Highly volatile from water. | Accumulates very little in the bodies of living organisms. | Not expected to leach through the soil or the sediment. |

# Section 13: Disposal Considerations

|  |
| --- |
| Dispose in accordance with all applicable regulations. Subject to disposal regulations: U.S. EPA 40 CFR 262. Hazardous Waste Number(s): D001. |

# Section 14: Transportation Information

## U.S. DOT 49 CFR 172.101

| Proper Shipping Name | ID Number | Hazard Class or Division | Packing Group | Labeling Requirements | Passenger Aircraft or Railcar Quantity Limitations | Cargo Aircraft Only Quantity Limitations | Additional Shipping Description |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Hexanes | UN1208 | 3 | II | 3 | 5 kg or L | N/A | N/A |

## Canadian Transportation of Dangerous Goods

|  |  |  |  |
| --- | --- | --- | --- |
| Shipping Name | UN Number | Class | Packing Group / Risk Group |
| Hexanes | UN1208 | 3 | II |

# Section 15: Regulatory Information

## U.S. Regulations

|  |  |  |
| --- | --- | --- |
| CERCLA Sections | SARA 355.30 | SARA 355.40 |
| 5000 LBS RQ | Not regulated. | Not regulated. |

## SARA 370.21

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Acute | Chronic | Fire | Reactive | Sudden Release |
| Yes | Yes | Yes | No | No |

## SARA 372.65

|  |
| --- |
| N-HEXANE |

## OSHA Process Safety

|  |
| --- |
| Not regulated. |

## State Regulations

|  |
| --- |
| CA Proposition 65 |
| Not regulated. |

## Canadian Regulations

|  |
| --- |
| WHMIS Classification |
| B2, D2A, D2B |

## National Inventory Status

|  |  |  |
| --- | --- | --- |
| US Inventory (TSCA) | TSCA 12b Export Notification | Canada Inventory (DSL/NDSL) |
| Listed on inventory. | Not listed. | Listed on DSL. |

# Section 16: Other Information

|  |
| --- |
| NFPA Rating |
| HEALTH=2 FIRE=3 REACTIVITY=0 |

0 = minimal hazard, 1 = slight hazard, 2 = moderate hazard, 3 = severe hazard, 4 = extreme hazard