|  |  |
| --- | --- |
| Metro Welding Supply Corp. logo | Safety Data SheetCarbon Dioxide |
|  |

# Section 1: Product and Company Identification

**Metro Welding Supply Corp.**

12620 Southfield Road

Detroit, MI 48223

(313) 834-1660 [phone]

(313) 835-3562 [fax]

http://www.metrowelding.com/

Product Code: Carbon Dioxide

# Section 2: Hazards Identification



**Danger**

## Hazard Classification:

Aspiration Hazard (Category 1)

Eye Effects (Category 2.B)

Gases Under Pressure

## Hazard Statements:

Causes eye irritation

Contains gas under pressure; may explode if heated

May be fatal if swallowed and enters airways

## Precautionary Statements

**Prevention:**

Wash thoroughly after handling.

**Response:**

Do NOT induce vomiting.

If in eyes: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing.

If swallowed: Rinse mouth. Do NOT induce vomiting.

Immediately call a poison center or doctor.

**Storage:**

Protect from sunlight.

Store in well-ventilated place.

Store locked up.

**Disposal:**

Dispose of contents and/or container in accordance with applicable regulations.

# Section 3: Composition/Information on Ingredients

| CAS # |
| --- |
| 124-38-9 |

| Chemical Substance | Chemical Family | Trade Names |
| --- | --- | --- |
| CARBON DIOXIDE, GAS | oxides of carbon | CARBONIC ACID GAS; CARBONIC ANHYDRIDE; CARBON DIOXIDE; CARBON OXIDE; UN 1013; CO2 |

# Section 4: First Aid Measures

| Skin Contact | Eye Contact | Ingestion | Inhalation | Note to Physicians |
| --- | --- | --- | --- | --- |
| If frostbite or freezing occur, immediately flush with plenty of lukewarm water (105-115 F; 41-46 C). DO NOT USE HOT WATER. If warm water is not available, gently wrap affected parts in blankets. Get immediate medical attention. | Contact with liquid: Immediately flush eyes with plenty of water for at least 15 minutes. Then get immediate medical attention. | Do not induce vomiting. | If adverse effects occur, remove to uncontaminated area. Give artificial respiration if not breathing. If breathing is difficult, oxygen should be administered by qualified personnel. Get immediate medical attention. | For inhalation, consider oxygen. |

# Section 5: Fire Fighting Measures

| Suitable Extinguishing Media | Products of Combustion | Protection of Firefighters |
| --- | --- | --- |
| Non-flammable | Non-flammable | * Any appropriate escape-type, self-contained breathing apparatus.
* Non-flammable
 |

# Section 6: Accidental Release Measures

| Personal Precautions | Environmental Precautions | Methods for Containment |
| --- | --- | --- |
| Keep unnecessary people away, isolate hazard area and deny entry. Ventilate closed spaces before entering. Do not touch spilled material. | Subject to California Safe Drinking Water and Toxic Enforcement Act of 1986 (Proposition 65). Keep out of
water supplies and sewers. | Stop leak if possible without personal risk.  |

| Methods for Cleanup | Other Information |
| --- | --- |
| Stop leak, evacuate, remove source of ignition.  | None |

# Section 7: Handling and Storage

| Handling | Storage |
| --- | --- |
| Subject to storage regulations: U.S. OSHA 29 CFR 1910.101. Keep separated from incompatible substances. | Store and handle in accordance with all current regulations and standards |

# Section 8: Exposure Controls/Personal Protection

| Exposure Guidelines |
| --- |
| CARBON DIOXIDE, GAS: CARBON DIOXIDE: 5000 ppm (9000 mg/m3) OSHA TWA 10000 ppm (18000 mg/m3) OSHA TWA (vacated by 58 FR 35338, June 30, 1993) 30000 ppm (54000 mg/m3) OSHA STEL (vacated by 58 FR 35338, June 30, 1993) 5000 ppm ACGIH TWA 30000 ppm ACGIH STEL 5000 ppm (9000 mg/m3) NIOSH recommended TWA 10 hour(s) 30000 ppm (54000 mg/m3) NIOSH recommended STEL |

## Engineering Controls

Handle only in fully enclosed systems.

| Eye Protection | Skin Protection | Respiratory Protection |
| --- | --- | --- |
| For the gas: Eye protection not required, but recommended. For the liquid: Wear splash resistant safety goggles. Contact lenses should not be worn. Provide an emergency eye wash fountain and quick drench shower in the immediate work area. | For the gas: Protective clothing is not required. For the liquid: Wear appropriate protective, cold insulating clothing. | Any appropriate escape-type, self-contained breathing apparatus. |

## General Hygiene considerations

* Avoid breathing vapor or mist
* Avoid contact with eyes and skin
* Wash thoroughly after handling and before eating or drinking

# Section 9: Physical and Chemical Properties

| Physical State | Appearance | Color | Change in Appearance | Physical Form | Odor | Taste |
| --- | --- | --- | --- | --- | --- | --- |
| Gas | Colorless | Colorless | N/A | Gas | Odorless | Acid taste |

| Flash Point | Flammability | Partition Coefficient | Autoignition Temperature | Upper Explosive Limits | Lower Explosive Limits |
| --- | --- | --- | --- | --- | --- |
| Not flammable | Not available | N/A | Nonflammable | Nonflammable | Nonflammable |

| Boiling Point | Freezing Point | Vapor Pressure | Vapor Density | Specific Gravity | Water Solubility | pH | Odor Threshold | Evaporation Rate | Viscosity |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Not available | -71 F (-57 C) @ 4000 mmHg | 43700 mmHg @ 21 C | 1.5 (Air=1) | 1.522 @ 21 C | Soluble | 3.7 (saturated aqueous solution) @ 101.3 kPa (carbonic acid) | Not available | Not applicable | 0.01657 cP @ 0 C |

| Molecular Weight | Molecular Formula | Density | Weight per Gallon | Volatility by Volume | Volatility | Solvent Solubility |
| --- | --- | --- | --- | --- | --- | --- |
| 44.01 | C-O2 | 0.114 | Not available | Not applicable | Not applicable | Soluble: Alcohol, acetone, hydrocarbons, organic solvents |

# Section 10: Stability and Reactivity

| Stability | Conditions to Avoid | Incompatible Materials |
| --- | --- | --- |
| Stable at normal temperatures and pressure. | Stable at normal temperatures and pressure. | Combustible materials, oxidizing materials, metal salts, reducing agents, metal carbide, metals, bases |

| Hazardous Decomposition Products | Possibility of Hazardous Reactions |
| --- | --- |
| Carbon monoxide | Will not polymerize. |

# Section 11: Toxicology Information

## Acute Effects

| Oral LD50 | Dermal LD50 | Inhalation |
| --- | --- | --- |
| Not established | Not established | Ringing in the ears, nausea, irregular heartbeat, headache, drowsiness, dizziness, tingling sensation, visual disturbances, suffocation, convulsions, coma |

| Eye Irritation | Skin Irritation | Sensitization |
| --- | --- | --- |
| Irritation, frostbite, blurred vision | Liquid: blisters, frostbite | Difficulty breathing |

## Chronic Effects

| Carcinogenicity | Mutagenicity | Reproductive Effects | Developmental Effects |
| --- | --- | --- | --- |
| Not available | Not established | Available. | No data |

# Section 12: Ecological Information

## Fate and Transport

|  |  |  |  |
| --- | --- | --- | --- |
| Eco toxicity | Persistence / Degradability | Bioaccumulation / Accumulation | Mobility in Environment |
| Fish toxicity: 150000 ug/L 48 day(s) (Mortality) Brown trout (Salmo trutta)Invertibrate toxicity: Not availableAlgal toxicity: Not availablePhyto toxicity: Not availableOther toxicity: Not available | Relatively non-persistent in the environment. Moderately volatile from water. | Accumulates very little in the bodies of living organisms. | Leaches through the soil |

# Section 13: Disposal Considerations

|  |
| --- |
| Dispose in accordance with all applicable regulations. |

# Section 14: Transportation Information

## U.S. DOT 49 CFR 172.101

| Proper Shipping Name | ID Number | Hazard Class or Division | Packing Group | Labeling Requirements | Passenger Aircraft or Railcar Quantity Limitations | Cargo Aircraft Only Quantity Limitations | Additional Shipping Description |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Carbon dioxide | UN1013 | 2.2 | Not applicable | 2.2 | 75 kg or L | 150kg | None |

## Canadian Transportation of Dangerous Goods

|  |  |  |  |
| --- | --- | --- | --- |
| Shipping Name | UN Number | Class | Packing Group / Risk Group |
| Carbon dioxide | UN1013 | 2.2 | Not applicable |

# Section 15: Regulatory Information

## U.S. Regulations

|  |  |  |
| --- | --- | --- |
| CERCLA Sections | SARA 355.30 | SARA 355.40 |
| Not regulated. | Not regulated. | Not regulated. |

## SARA 370.21

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Acute | Chronic | Fire | Reactive | Sudden Release |
| Yes | No | No | No | Yes |

## SARA 372.65

|  |
| --- |
| Not regulated. |

## OSHA Process Safety

|  |
| --- |
| Not regulated. |

## State Regulations

|  |
| --- |
| CA Proposition 65 |
| Not regulated. |

## Canadian Regulations

|  |
| --- |
| WHMIS Classification |
| A |

## National Inventory Status

|  |  |  |
| --- | --- | --- |
| US Inventory (TSCA) | TSCA 12b Export Notification | Canada Inventory (DSL/NDSL) |
| Listed on inventory. | Not listed. | Listed on inventory. |

# Section 16: Other Information

|  |
| --- |
| NFPA Rating |
| HEALTH=2 FIRE=0 REACTIVITY=0 |

0 = minimal hazard, 1 = slight hazard, 2 = moderate hazard, 3 = severe hazard, 4 = extreme hazard