|  |  |
| --- | --- |
| Metro Welding Supply Corp. logo | Safety Data SheetEthyl Chloride |
|  |

# Section 1: Product and Company Identification

**Metro Welding Supply Corp.**

12620 Southfield Road

Detroit, MI 48223

(313) 834-1660 [phone]

(313) 835-3562 [fax]

http://www.metrowelding.com/

Product Code: Ethyl Chloride

# Section 2: Hazards Identification



**Danger**

## Hazard Classification:

Acute Gas Inhale Toxicity (Category 2)

Aspiration Hazard (Category 1)

Carcinogenicity (Category 1.B)

Eye Effects (Category 2.B)

Flammable (Category 1)

Flammable Aerosol (Category 1)

Gases Under Pressure

## Hazard Statements:

Causes eye irritation

Contains gas under pressure; may explode if heated

Extremely flammable aerosol

Extremely flammable gas

Fatal if inhaled

May be fatal if swallowed and enters airways

May cause cancer

## Precautionary Statements

**Prevention:**

Do not breathe dust/fume/gas/mist/ vapors/spray..

[In case of inadequate ventilation] wear respiratory protection.

Do not handle until all safety precautions have been read and understood.

Wash thoroughly after handling.

Use only outdoors or in a well-ventilated area.

Wear protective gloves, protective clothing, eye protection and face protection.

Obtain special instructions before use.

Keep away from heat/sparks/open flames/hot surfaces. - No smoking.

Pressurized container: Do not pierce or burn, even after use.

Do not spray on an open flame or other ignition source.

**Response:**

Eliminate all ignition sources if safe to do so.

Immediately call a poison center or doctor.

Leaking gas fire: Do not extinguish, unless leak can be stopped safely.

Do NOT induce vomiting.

Specific treatment is urgent.

If swallowed: Rinse mouth. Do NOT induce vomiting.

If exposed or concerned: Get medical advice/attention.

If in eyes: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing.

If inhaled: Remove person to fresh air and keep comfortable for breathing.

**Storage:**

Store in a well-ventilated place. Keep container tightly closed.

Protect from sunlight.

Store locked up.

Do not expose to temperatures exceeding 50C/122F.

**Disposal:**

Dispose of contents and/or container in accordance with applicable regulations.

# Section 3: Composition/Information on Ingredients

| CAS # |
| --- |
| 75-00-3 |

| Chemical Substance | Chemical Family | Trade Names |
| --- | --- | --- |
| ETHYL CHLORIDE | halogenated, aliphatic | CHLOROETHANE; MONOCHLOROETHANE; MURIATIC ETHER; KELENE; HYDROCHLORIC ETHER; ETHER HYDROCHLORIC; ETHER MURIATIC; NARCOTILE; AETHYLIS; CHELEN; CHLORETHYL; CHLORIDUM; CHLORYL; CHLORYL ANESTHETIC; ETHER CHLORATUS; AETHYLIS CHLORIDUM; STCC 4908162; UN 1037; C2H5CL |

# Section 4: First Aid Measures

| Skin Contact | Eye Contact | Ingestion | Inhalation | Note to Physicians |
| --- | --- | --- | --- | --- |
| If frostbite or freezing occur, immediately flush with plenty of lukewarm water (105-115 F; 41-46 C). DO NOT USE HOT WATER. If warm water is not available, gently wrap affected parts in blankets. Get immediate medical attention. | Flush eyes with plenty of water for at least 15 minutes. Then get immediate medical attention. | Contact local poison control center or physician immediately. Never make an unconscious person vomit or drink fluids. When vomiting occurs, keep head lower than hips to help prevent aspiration. If person is unconscious, turn head to side. Get medical attention. | If adverse effects occur, remove to uncontaminated area. Give artificial respiration if not breathing. If breathing is difficult, oxygen should be administered by qualified personnel. Get immediate medical attention. | Not available |

# Section 5: Fire Fighting Measures

| Suitable Extinguishing Media | Products of Combustion | Protection of Firefighters |
| --- | --- | --- |
| Regular dry chemical, carbon dioxide, regular foam  | Hydrogen chloride gas, phosgene. | * Any self-contained breathing apparatus that has a full facepiece and is operated in a pressure-demand or other positive-pressure mode. Use chemical protective clothing.
* Not available
 |

# Section 6: Accidental Release Measures

| Personal Precautions | Environmental Precautions | Methods for Containment |
| --- | --- | --- |
| Keep unnecessary people away, isolate hazard area and deny entry. | Avoid heat, flames, sparks and other sources of ignition.  | Stop leak if possible without personal risk. Reduce vapors with water spray. |

| Methods for Cleanup | Other Information |
| --- | --- |
| Small spills: Absorb with sand or other non-combustible material. Collect spilled material in appropriate container for disposal. Large spills: Dike for later disposal. Remove sources of ignition.  | Notify Local Emergency Planning Committee and State Emergency Response Commission for release greater than or equal to RQ (U.S. SARA Section 304). If release occurs in the U.S. and is reportable under CERCLA Section 103, notify the National Response Center at (800)424-8802 (USA) or (202)426-2675 (USA). Subject to California Safe Drinking Water and Toxic Enforcement Act of 1986 (Proposition 65).  |

# Section 7: Handling and Storage

| Handling | Storage |
| --- | --- |
| Store and handle in accordance with all current regulations and standards. Subject to storage regulations: U.S. OSHA 29 CFR 1910.101. Grounding and bonding required. Protect from physical damage. Store outside or in a detached building. Store with flammable liquids. Keep separated from incompatible substances. Avoid contact with light. Store in a cool, dry place. Store in a well-ventilated area. Keep separated from incompatible substances. | Avoid contact with eyes, skin and clothing. Keep container closed. Use only with adequate ventilation. Keep away from heat, sparks and flame. To avoid fire, minimize ignition sources. Use explosion-proof electrical (ventilating, lighting and material handling) equipment. Do not puncture or incinerate container. Wash thoroughly after handling. High pressure gas. Use equipment rated for cylinder pressure. Close valve after each use and when empty. |

# Section 8: Exposure Controls/Personal Protection

| Exposure Guidelines |
| --- |
| ETHYL CHLORIDE: 1000 ppm (2600 mg/m3) OSHA TWA 100 ppm ACGIH TWA (skin) NIOSH (handle with caution in workplace) |

## Engineering Controls

Handle only in fully enclosed systems.

| Eye Protection | Skin Protection | Respiratory Protection |
| --- | --- | --- |
| For the gas: Eye protection not required, but recommended. For the liquid: Wear splash resistant safety goggles. Contact lenses should not be worn. Provide an emergency eye wash fountain and quick drench shower in the immediate work area. | For the gas: Protective clothing is not required. For the liquid: Wear appropriate protective, cold insulating clothing. | Any self-contained breathing apparatus that has a full facepiece and is operated in a pressure-demand or other positive-pressure mode. Use chemical protective clothing. |

## General Hygiene considerations

* Avoid breathing vapor or mist
* Avoid contact with eyes and skin
* Wash thoroughly after handling and before eating or drinking

# Section 9: Physical and Chemical Properties

| Physical State | Appearance | Color | Change in Appearance | Physical Form | Odor | Taste |
| --- | --- | --- | --- | --- | --- | --- |
| Gas | Colorless | Colorless | N/A | Gas | Pungent, ether-like odor | Burning taste |

| Flash Point | Flammability | Partition Coefficient | Autoignition Temperature | Upper Explosive Limits | Lower Explosive Limits |
| --- | --- | --- | --- | --- | --- |
| -58 F (-50 C) (CC) | Not available | Not available | 966 F (519 C) | 0.154 | 0.038 |

| Boiling Point | Freezing Point | Vapor Pressure | Vapor Density | Specific Gravity | Water Solubility | pH | Odor Threshold | Evaporation Rate | Viscosity |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 54 F (12 C) | -213 F (-136 C) | 1000 mmHg @ 20 C | 2.2 (Air=1) | 0.9 | 0.6% | Not applicable | 4.2 ppm (method not specified) (10); 140 ppm (50% detection); 680 ppm (100% detection) | Not applicable | 0.26 mPa.s (0.26 centipoise) @ 20 C |

| Molecular Weight | Molecular Formula | Density | Weight per Gallon | Volatility by Volume | Volatility | Solvent Solubility |
| --- | --- | --- | --- | --- | --- | --- |
| 64.52 | C2-H5-CL | 0.1649 | Not available | Not available | Not applicable | Soluble: Alcohol, ether, organic solvents |

# Section 10: Stability and Reactivity

| Stability | Conditions to Avoid | Incompatible Materials |
| --- | --- | --- |
| Stable at normal temperatures and pressure. May react on contact with water. May release toxic and/or flammable gases. | Stable at normal temperatures and pressure. May react on contact with water. May release toxic and/or flammable gases. | Metals, oxidizing materials, water, aluminum, powdered metals |

| Hazardous Decomposition Products | Possibility of Hazardous Reactions |
| --- | --- |
| Acid halides, phosgene, hydrochloric acid | Will not polymerize. |

# Section 11: Toxicology Information

## Acute Effects

| Oral LD50 | Dermal LD50 | Inhalation |
| --- | --- | --- |
| (LC50): 80 ppm 4 hour(s) [Rat]. | Not available | Irritation, blisters, blurred vision, nausea, vomiting, irregular heartbeat, headache, sore throat, frostbite, symptoms of drunkenness, disorientation, kidney damage, liver damage |

| Eye Irritation | Skin Irritation | Sensitization |
| --- | --- | --- |
| Irritation, blurred vision | Irritation, blisters, frostbite | Eye irritation, central nervous system depression |

## Chronic Effects

| Carcinogenicity | Mutagenicity | Reproductive Effects | Developmental Effects |
| --- | --- | --- | --- |
| IARC: Human No Adequate Data, Animal Limited Evidence, Group 3; ACGIH: A3 -Confirmed Animal Carcinogen | Available. | Available. | No data |

# Section 12: Ecological Information

## Fate and Transport

|  |  |  |  |
| --- | --- | --- | --- |
| Eco toxicity | Persistence / Degradability | Bioaccumulation / Accumulation | Mobility in Environment |
| Fish toxicity: Not availableInvertibrate toxicity: Not availableAlgal toxicity: Not availablePhyto toxicity: Not availableOther toxicity: Not available | 53- 91% degradation in 28 days of incubation) | None | Not available |

# Section 13: Disposal Considerations

|  |
| --- |
| Subject to disposal regulations: U.S. EPA 40 CFR 262. Hazardous Waste Number(s): D001. Dispose in accordance with all applicable regulations. |

# Section 14: Transportation Information

## U.S. DOT 49 CFR 172.101

| Proper Shipping Name | ID Number | Hazard Class or Division | Packing Group | Labeling Requirements | Passenger Aircraft or Railcar Quantity Limitations | Cargo Aircraft Only Quantity Limitations | Additional Shipping Description |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Ethyl chloride | UN1037 | 2.1 | Not applicable | 2.1 | Forbidden | 150 kg | None |

## Canadian Transportation of Dangerous Goods

|  |  |  |  |
| --- | --- | --- | --- |
| Shipping Name | UN Number | Class | Packing Group / Risk Group |
| Ethyl chloride | UN1037 | 2.1 | Not applicable |

# Section 15: Regulatory Information

## U.S. Regulations

|  |  |  |
| --- | --- | --- |
| CERCLA Sections | SARA 355.30 | SARA 355.40 |
| 100 LBS RQ | Not regulated. | Not regulated. |

## SARA 370.21

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Acute | Chronic | Fire | Reactive | Sudden Release |
| Yes | No | Yes | Yes | No |

## SARA 372.65

|  |
| --- |
| CHLOROETHANE (ETHYL CHLORIDE) |

## OSHA Process Safety

|  |
| --- |
| Not regulated. |

## State Regulations

|  |
| --- |
| CA Proposition 65 |
| Known to the state of California to cause the following: Chloroethane (Ethyl chloride) Cancer (Jul 01, 1990) |

## Canadian Regulations

|  |
| --- |
| WHMIS Classification |
| A, B1 |

## National Inventory Status

|  |  |  |
| --- | --- | --- |
| US Inventory (TSCA) | TSCA 12b Export Notification | Canada Inventory (DSL/NDSL) |
| Listed on inventory. | Not listed. | Not determined. |

# Section 16: Other Information

|  |
| --- |
| NFPA Rating |
| HEALTH=2 FIRE=4 REACTIVITY=0 |

0 = minimal hazard, 1 = slight hazard, 2 = moderate hazard, 3 = severe hazard, 4 = extreme hazard