|  |  |
| --- | --- |
| Metro Welding Supply Corp. logo | Safety Data SheetSulfur Hexafluoride |
|  |

# Section 1: Product and Company Identification

**Metro Welding Supply Corp.**

12620 Southfield Road

Detroit, MI 48223

(313) 834-1660 [phone]

(313) 835-3562 [fax]

http://www.metrowelding.com/

Product Code: Sulfur Hexafluoride

# Section 2: Hazards Identification



**Danger**

## Hazard Classification:

Aspiration Hazard (Category 1)

Gases Under Pressure

## Hazard Statements:

Contains gas under pressure; may explode if heated

May be fatal if swallowed and enters airways

## Precautionary Statements

**Response:**

Do NOT induce vomiting.

If swallowed: Rinse mouth. Do NOT induce vomiting.

Immediately call a poison center or doctor.

**Storage:**

Protect from sunlight.

Store in well-ventilated place.

Store locked up.

**Disposal:**

Dispose of contents and/or container in accordance with applicable regulations.

# Section 3: Composition/Information on Ingredients

| CAS # |
| --- |
| 2551-62-4 |

| Chemical Substance | Chemical Family | Trade Names |
| --- | --- | --- |
| SULFUR HEXAFLUORIDE | inorganic, gas | SULFUR FLUORIDE; SULPHUR HEXAFLUORIDE; ELEGAS; UN 1080; SF6 |

# Section 4: First Aid Measures

| Skin Contact | Eye Contact | Ingestion | Inhalation | Note to Physicians |
| --- | --- | --- | --- | --- |
| Wash exposed skin with soap and water. | Flush eyes with plenty of water. | If a large amount is swallowed, get medical attention. | If adverse effects occur, remove to uncontaminated area. Give artificial respiration if not breathing. If breathing is difficult, oxygen should be administered by qualified personnel. Get immediate medical attention. | For inhalation, consider oxygen. |

# Section 5: Fire Fighting Measures

| Suitable Extinguishing Media | Products of Combustion | Protection of Firefighters |
| --- | --- | --- |
| Non-flammable. Use suitable extinguishing media for surrounding fire.  | Thermal decomposition products or combustion: fluorinated compounds, oxides of sulfur, sulfur compounds, hydrogen fluoride, hydrogen sulfide | * Respiratory protection may be needed for frequent or heavy exposure. Any self-contained breathing apparatus with a full facepiece.
* Respiratory protection may be needed for frequent or heavy exposure. Any self-contained breathing apparatus with a full facepiece.
* Protective material types: leather
 |

# Section 6: Accidental Release Measures

| Personal Precautions | Environmental Precautions | Methods for Containment |
| --- | --- | --- |
| Keep unnecessary people away, isolate hazard area and deny entry. Stay upwind and keep out of low areas. | Prevent environmental contamination. | Stop leak if possible without personal risk. |

| Methods for Cleanup | Other Information |
| --- | --- |
| Evacuate area, stop leak. Contact emergency personnel. | None |

# Section 7: Handling and Storage

| Handling | Storage |
| --- | --- |
| Store and handle in accordance with all current regulations and standards. Store below 49 C. Avoid shock. Store in a well-ventilated area. Store in a tightly closed container. Keep away from heat, sparks and flame. Store in a cool, dry place. Subject to storage regulation: U.S. OSHA 29 CFR 1910.101. |  Keep separated from incompatible substances. Secure to prevent tipping.  |

# Section 8: Exposure Controls/Personal Protection

| Exposure Guidelines |
| --- |
| SULFUR HEXAFLUORIDE: 1000 ppm (6000 mg/m3) OSHA TWA 1000 ppm ACGIH TWA 1000 ppm (6000 mg/m3) NIOSH recommended TWA 10 hour(s) |

## Engineering Controls

Handle only in fully enclosed systems.

| Eye Protection | Skin Protection | Respiratory Protection |
| --- | --- | --- |
| Wear splash resistant safety goggles with a face shield. Provide an emergency eye wash fountain and quick drench shower in the immediate work area. | Protective clothing is not required. | Respiratory protection may be needed for frequent or heavy exposure. Any self-contained breathing apparatus with a full facepiece. |

## General Hygiene considerations

* Avoid breathing vapor or mist
* Avoid contact with eyes and skin
* Wash thoroughly after handling and before eating or drinking

# Section 9: Physical and Chemical Properties

| Physical State | Appearance | Color | Change in Appearance | Physical Form | Odor | Taste |
| --- | --- | --- | --- | --- | --- | --- |
| Gas | Clear | Colorless | N/A | Gas | Odorless | N/A |

| Flash Point | Flammability | Partition Coefficient | Autoignition Temperature | Upper Explosive Limits | Lower Explosive Limits |
| --- | --- | --- | --- | --- | --- |
| Not flammable | Not available | 1.68 (log = 0.226) | Nonflammable | Nonflammable | Nonflammable |

| Boiling Point | Freezing Point | Vapor Pressure | Vapor Density | Specific Gravity | Water Solubility | pH | Odor Threshold | Evaporation Rate | Viscosity |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Not available | -58.9 F (-50.5 C) | 16548 mmHg @ 20 C | 5.1 (Air=1) | 1.68 | Slightly soluble | Not applicable | Not available | Not applicable | 0.0156 cP @ 25 C |

| Molecular Weight | Molecular Formula | Density | Weight per Gallon | Volatility by Volume | Volatility | Solvent Solubility |
| --- | --- | --- | --- | --- | --- | --- |
| 146.06 | F6-S | 0.3847 | Not available | 1 | 1 | Soluble: Alcohol, ether, potassium hydroxide solutions, transformer oil |

# Section 10: Stability and Reactivity

| Stability | Conditions to Avoid | Incompatible Materials |
| --- | --- | --- |
| Stable at normal temperatures and pressure. | Stable at normal temperatures and pressure. | Combustible materials, metals, oxidizing materials |

| Hazardous Decomposition Products | Possibility of Hazardous Reactions |
| --- | --- |
| Fluorinated compounds, oxides of sulfur, sulfur compounds, hydrogen fluoride, hydrogen sulfide | Will not polymerize. |

# Section 11: Toxicology Information

## Acute Effects

| Oral LD50 | Dermal LD50 | Inhalation |
| --- | --- | --- |
| Not available | Not available | Nausea, vomiting, difficulty breathing, dizziness, fatigue, emotional disturbances, tingling sensation, suffocation, convulsions, coma |

| Eye Irritation | Skin Irritation | Sensitization |
| --- | --- | --- |
| No information on significant adverse effects | No information on significant adverse effects | Difficulty breathing |

## Chronic Effects

| Carcinogenicity | Mutagenicity | Reproductive Effects | Developmental Effects |
| --- | --- | --- | --- |
| Not available | Not available | Not available | No data |

# Section 12: Ecological Information

## Fate and Transport

|  |  |  |  |
| --- | --- | --- | --- |
| Eco toxicity | Persistence / Degradability | Bioaccumulation / Accumulation | Mobility in Environment |
| Fish toxicity: Not availableInvertibrate toxicity: Not availableAlgal toxicity: Not availablePhyto toxicity: Not availableOther toxicity: Not available | Highly volatile from water. | Not available | Leaches through the soil or the sediment at a moderate rate. |

# Section 13: Disposal Considerations

|  |
| --- |
| Dispose in accordance with all applicable regulations. |

# Section 14: Transportation Information

## U.S. DOT 49 CFR 172.101

| Proper Shipping Name | ID Number | Hazard Class or Division | Packing Group | Labeling Requirements | Passenger Aircraft or Railcar Quantity Limitations | Cargo Aircraft Only Quantity Limitations | Additional Shipping Description |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Sulfur hexafluoride | UN1080 | 2.2 | Not applicable | 2.2 | 75 kg or L | 150 kg | N/A |

## Canadian Transportation of Dangerous Goods

|  |  |  |  |
| --- | --- | --- | --- |
| Shipping Name | UN Number | Class | Packing Group / Risk Group |
| Sulfur hexafluoride | UN1080 | 2.2 | Not applicable |

# Section 15: Regulatory Information

## U.S. Regulations

|  |  |  |
| --- | --- | --- |
| CERCLA Sections | SARA 355.30 | SARA 355.40 |
| Not regulated. | Not regulated. | Not regulated. |

## SARA 370.21

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Acute | Chronic | Fire | Reactive | Sudden Release |
| Yes  | Yes | No | No | Yes |

## SARA 372.65

|  |
| --- |
| Not regulated. |

## OSHA Process Safety

|  |
| --- |
| Not regulated. |

## State Regulations

|  |
| --- |
| CA Proposition 65 |
| Not regulated. |

## Canadian Regulations

|  |
| --- |
| WHMIS Classification |
| A. |

## National Inventory Status

|  |  |  |
| --- | --- | --- |
| US Inventory (TSCA) | TSCA 12b Export Notification | Canada Inventory (DSL/NDSL) |
| Listed on inventory. | Not listed. | Not determined. |

# Section 16: Other Information

|  |
| --- |
| NFPA Rating |
| HEALTH=1 FIRE=0 REACTIVITY=0 |

0 = minimal hazard, 1 = slight hazard, 2 = moderate hazard, 3 = severe hazard, 4 = extreme hazard